{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":67,"n_cols":6,"rows_kept":67,"merged":[[0,0,1,5],[3,0,9,0],[3,1,9,1],[3,2,9,2],[3,4,16,4],[3,5,16,5],[10,0,16,0],[10,1,16,1],[10,2,16,2],[55,4,60,4],[64,4,66,4]],"flags":["formulas_cached_only"]}
["安徽昊源化工集团有限公司颍东新材料产业园分公司2022年度环境检测计划"]
[]
["序号","排放口编号","检测点位","检测项目","备注","执行标准"]
[1,"DA001","一期锅炉固定污染源烟气CEMS在线比对监测","二氧化硫","停炉则取消"]
[{"$nulls":3},"氮氧化物"]
[{"$nulls":3},"含氧量"]
[{"$nulls":3},"烟尘（颗粒物）超低"]
[{"$nulls":3},"流速"]
[{"$nulls":3},"烟温"]
[{"$nulls":3},"湿度"]
[2,"DA002","二期锅炉固定污染源烟气CEMS在线比对监测","二氧化硫"]
[{"$nulls":3},"氮氧化物"]
[{"$nulls":3},"含氧量"]
[{"$nulls":3},"烟尘（颗粒物）超低"]
[{"$nulls":3},"流速"]
[{"$nulls":3},"烟温"]
[{"$nulls":3},"湿度"]
[3,"DA001","一期锅炉废气排放口","颗粒物（超低）、二氧化硫、氮氧化物、林格曼黑度、汞及其化合物","停炉则取消","火电厂大气污染物排放标准GB 13223-2011:黑度：1，氮氧化物：50，汞及其化合物0.03，二氧化硫：35.颗粒物：10"]
[4,"DA002","二期锅炉废气排放口","颗粒物（超低）、二氧化硫、氮氧化物、林格曼黑度、汞及其化合物","停炉则取消","火电厂大气污染物排放标准GB 13223-2011:黑度：1，氮氧化物：50，汞0.03，二氧化硫：35.颗粒物：10"]
[5,"DA003","蒸汽过热炉废气排放口","VOCs、二氧化硫、氮氧化物、甲苯、苯乙烯、苯、颗粒物、乙苯","苯乙烯停车取消","石油化学工业污染物排放标准GB 31571-2015：苯乙烯50，乙苯：100，VOC：120，苯：4，甲苯：15，颗粒物：20.氮氧化物：100，二氧化硫：20"]
[6,"DA011","2#灰库","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[7,"DA004-DA009","筒仓废气排放口1#-6#（6个）","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[8,"DA057-DA059、","筒仓废气排放口7#-9#（3个）","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[9,"DA051-DA053","筒仓废气排放口10#-12#（3个）","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[10,"DA010","粉煤锁斗过滤器排放口 ","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[11,"DA012-DA014","碎煤机排气筒1#-3#","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[12,"DA015","3#锅炉煤仓排放口A","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[13,"DA016-DA019","1#、2#、3#、4#煤仓排气筒","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[14,"DA021","一期气化粉煤加压输送进料系统粉煤仓排气筒","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[15,"DA024","3#锅炉煤仓排放口B","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[16,"DA029","3#锅炉煤仓排放口","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[17,"DA031","4#锅炉煤仓排放口B","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[18,"DA035","4#锅炉煤仓排放口C","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[19,"DA038","4#灰库","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[20,"DA040","3#灰库","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[21,"DA041","2#灰库","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[22,"DA042","1#灰库","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[23,"DA039","一期气化A炉磨煤干燥排气筒","颗粒物、氮氧化物","1次/季度","石油化学工业污染物排放标准GB 31571-2015：氮氧化物：180，大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[24,"DA043","一期气化B炉磨煤干燥排气筒","颗粒物、氮氧化物","1次/季度","石油化学工业污染物排放标准GB 31571-2015：氮氧化物：180，大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[25,"DA044、DA045","1#、2#渣仓","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[26,"DA047","二期气化粉煤加压输送进料系统粉煤仓排气筒","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[27,"DA048","尿素储运及包装除尘装置排气筒","颗粒物 ","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[28,"DA050","尿素尾气酸洗塔","氨","1次/季度","上海市《恶臭（异味）污染物排放标准》，氨：30"]
[29,"DA060","二甘醇氨真空泵排气筒","挥发性有机物","1次/季度","石油化学工业污染物排放标准GB 31571-2015 VOCs:120"]
[30,"DA062","乙二醇真空泵出口水洗塔排气筒","挥发性有机物、甲醇","目前尚未开车正常。待正常后通知","石油化学工业污染物排放标准GB 31571-2015 VOCs:120，甲醇：50"]
[31,"DA036","硫回收废气排放口","SO2、硫化氢  硫酸雾、氮氧化物","1次/季度","石油炼制工业污染物排放标准GB 31570-2015：氮氧化物：150，二氧化硫：100，硫酸雾：5；上海市《恶臭（异味）污染物排放标准》，硫化氢：50"]
[32,"DA020、DA078","一期、二期烟气脱硫硫酸铵放空（两个点）","颗粒物","1次/季度","大气污染物综合排放标准GB16297-1996  颗粒物：120"]
[33,"DA083","甲醇罐区闪蒸洗涤吸收塔排放口","甲醇","1次/季度","石油化学工业污染物排放标准GB 31571-2015 甲醇：50"]
[34,"DA081","N-甲基氧化吗啉吸收塔排放口","挥发性有机物","1次/季度","石油化学工业污染物排放标准GB 31571-2015 VOCs:120"]
[35,"DA077、DA082","一期、二期甲醇洗尾气排放口","臭气浓度、硫化氢、甲醇","1次/季度","上海市《恶臭（异味）污染物排放标准》，硫化氢：5；石油化学工业污染物排放标准GB 31571-2015，甲醇：50；恶臭污染物排放标准 GB 14554-93,臭气浓度60000"]
[36,"DA079","氨合成尾气排气筒","氨","1次/季度","上海市《恶臭（异味）污染物排放标准》，氨：30"]
[37,"DA086","二期气化A炉磨煤干燥排放口","颗粒物、氮氧化物","1次/季度","石油化学工业污染物排放标准GB 31571-2015：氮氧化物：180，大气污染物综合排放标准GB16297-1996  颗粒物：122"]
[38,"DA088","二期气化B炉磨煤干燥排放口","颗粒物、氮氧化物","1次/季度","石油化学工业污染物排放标准GB 31571-2015：氮氧化物：180，大气污染物综合排放标准GB16297-1996  颗粒物：122"]
[39,null,"企业边界（无组织）","硫化氢、氨、臭气浓度、非甲烷总烃","1次/季度","厂界的恶臭需从严执行上海市的恶臭污染物排放标准"]
[40,null,"企业边界（无组织）","甲醇、颗粒物","1次/年","厂界的恶臭需从严执行上海市的恶臭污染物排放标准"]
[41,null,"工业自来水（昊颍环保科技公司）","硫酸盐（以SO42-计）,溶解性总固体、pH值、悬浮物、五日生化需氧量、化学需氧量、氨氮（NH3-N）、总磷（以P计）浊度、色度、铁、锰、氯离子、二氧化硅、总硬度、总碱度、石油类、阴离子表面活性剂、余氯、粪大肠菌群","1次/季度","城市污水再生利用工业用水水质（GB/T19923-2005)"]
[42,"DW002","雨水排口（比对）","pH、氨氮、COD、总氮、总磷",null,"合成氨工业水污染物排放标准 GB 13458-2013"]
[43,"DW001","污水排口（比对）","氨氮、COD",null,"合成氨工业水污染物排放标准 GB 13458-2013"]
[44,null,"厂界噪声","噪声(昼夜）",null,"工业企业厂界环境噪声排放标准三类"]
[45,null,"废水（园区污水处理厂来浓水）","氯离子,硫酸盐（以SO42-计）,溶解性总固体、pH值、总硬度、悬浮物、电导率、五日生化需氧量、化学需氧量、总汞、烷基汞、总砷、总铅、总氮（以N计）、氨氮（NH3-N）、总磷（以P计）、硫化物、硫酸盐（以SO42-计）、氰化物、氟化物"]
[46,"DW001","废水（去园区污水处理厂）","氨氮、色度、浑浊度、全盐量、电导率、五日生化需氧量、总有机碳、硫酸盐（以SO42-计）、氰化物、氯离子、烷基汞",null,"合成氨工业水污染物排放标准 GB 13458-2013"]
[47,"DW001","废水（去园区污水处理厂）","溶解性总固体、总硬度、悬浮物、总氮（以N计）、总磷（以P计）、硫化物、石油类、挥发酚","1次/月","合成氨工业水污染物排放标准 GB 13458-2013"]
[48,null,"厂区土壤（18个点）","pH、总汞、总镉、总铬、总砷、总铅、总镍、总铜、苯、甲苯、乙苯、苯乙烯","1次/年"]
[49,null,"地下水（7个点）","pH、总汞、总镉、总铬、六价铬、总砷、总铅、总镍、总铜、挥发酚","1次/年"]
[50,null,"循环水（1#、2#、3#、4#、5#、6#）","TOC","1次/季度"]
[51,null,"周边水质","氨氮、COD、总氮、总磷、TDS"]
[52,null,"充装栈台洗涤塔放空气","VOC、甲醇"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}